# This is my beautiful, main, header

In our logging system every running copy of the receiver program will get the messages. That way we'll be able to run one receiver and direct the logs to disk; and at the same time we'll be able to run another receiver and see the logs on the screen.

Essentially, published **log messages** are going to be broadcast to all the receivers.

|  |  |
| --- | --- |
| First cell | Second cell |
| Third cell | Fouth cell |
| Fifth | Sixth |

What about now?

And now?